Agora RTC Objective-C API Reference Refactor

Data Fields
ContentInspectModule Struct Reference

## Data Fields
CONTENT_INSPECT_TYPE | type
unsigned int | interval
base::VIDEO_MODULE_POSITION | position

## Constructor & Destructor Documentation

## ◆ ContentInspectModule()

ContentInspectModule | ( |  | ) |
| inline

## Field Documentation

## ◆ type

CONTENT_INSPECT_TYPE type

Types of functional module. See `CONTENT_INSPECT_TYPE`.

## ◆ interval

unsigned int interval

The frequency (s) of video screenshot and upload. The value should be set as larger than 0. The default value is 0, the SDK does not take screenshots. Agora recommends that you set the value as 10; you can also adjust it according to your business needs.

## ◆ position

base::VIDEO_MODULE_POSITION position

The position of the video observer. See `VIDEO_MODULE_POSITION`.