Agora RTC Objective-C API Reference Refactor

Data Fields
MultipathStats Struct Reference

## Data Fields
uint32_t | lanTxBytes
uint32_t | lanRxBytes
uint32_t | wifiTxBytes
uint32_t | wifiRxBytes
uint32_t | mobileTxBytes
uint32_t | mobileRxBytes
int | activePathNum
const PathStats * | pathStats

## Detailed Description

Since
  4.6.0

## Constructor & Destructor Documentation

## ◆ MultipathStats()

MultipathStats | ( |  | ) |
| inline

## Field Documentation

## ◆ lanTxBytes

uint32_t lanTxBytes

The total number of bytes sent over the LAN path.

## ◆ lanRxBytes

uint32_t lanRxBytes

The total number of bytes received over the LAN path.

## ◆ wifiTxBytes

uint32_t wifiTxBytes

The total number of bytes sent over the Wi-Fi path.

## ◆ wifiRxBytes

uint32_t wifiRxBytes

The total number of bytes received over the Wi-Fi path.

## ◆ mobileTxBytes

uint32_t mobileTxBytes

The total number of bytes sent over the mobile network path.

## ◆ mobileRxBytes

uint32_t mobileRxBytes

The total number of bytes received over the mobile network path.

## ◆ activePathNum

int activePathNum

The number of active transmission paths.

## ◆ pathStats

const PathStats* pathStats

An array of statistics for each active transmission path. See `PathStats`.