Agora RTC Objective-C API Reference Refactor

Data Fields
LastmileProbeConfig Struct Reference

## Data Fields
bool | probeUplink
bool | probeDownlink
unsigned int | expectedUplinkBitrate
unsigned int | expectedDownlinkBitrate

## Field Documentation

## ◆ probeUplink

bool probeUplink

Sets whether to test the uplink network. Some users, for example, the audience members in a LIVE_BROADCASTING channel, do not need such a test.

- `true`: Test the uplink network.
- `false`: Do not test the uplink network.

## ◆ probeDownlink

bool probeDownlink

Sets whether to test the downlink network:

- `true`: Test the downlink network.
- `false`: Do not test the downlink network.

## ◆ expectedUplinkBitrate

unsigned int expectedUplinkBitrate

The expected maximum uplink bitrate (bps) of the local user. The value range is [100000, 5000000]. Agora recommends referring to `setVideoEncoderConfiguration` to set the value.

## ◆ expectedDownlinkBitrate

unsigned int expectedDownlinkBitrate

The expected maximum downlink bitrate (bps) of the local user. The value range is [100000,5000000].