Agora RTC Objective-C API Reference Refactor

Data Fields
RtmpStreamingAudioConfiguration Struct Reference

## Data Fields
int | sampleRateHz
int | bytesPerSample
int | numberOfChannels
int | bitrate

## Detailed Description

Configurations for the RTMP audio stream.

## Constructor & Destructor Documentation

## ◆ RtmpStreamingAudioConfiguration()

RtmpStreamingAudioConfiguration | ( |  | ) |
| inline

## Field Documentation

## ◆ sampleRateHz

int sampleRateHz

Sampling rate (Hz). The default value is 44100 (i.e. 44.1kHz).

## ◆ bytesPerSample

int bytesPerSample

Number of bytes per sample. The default value is 2 (i.e. 16-bit PCM).

## ◆ numberOfChannels

int numberOfChannels

Number of channels. The default value is 1 (i.e. mono).

## ◆ bitrate

int bitrate

The target bitrate (Kbps) of the output audio stream to be published. The default value is 48 Kbps.